# Checklist "Normal Procedures" for Gulfstream IV-SP V1.11 by ghansen 

sw_checklist:// Gulfstream IV-SP (V1.11) Checklist \\
sw_itemvoid: ======================================
sw_itemvoid:                            NORMAL PROCEDURES
sw_itemvoid:                                     Version 1.1
sw_itemvoid:                                    by Belgarath
sw_itemvoid:
sw_itemvoid:                              Fly safe and have fun...
sw_itemvoid: ======================================
sw_itemvoid: Thanks to ghansen for his incredible work with this airplane.


sw_checklist: APU Start:APU Start
sw_item: Cabin Door|CLOSED:sim/cockpit2/switches/custom_slider_on:0
sw_item: Parking Brake|SET:sim/flightmodel/controls/parkbrake:1
sw_item: HP Fuel Cocks|SHUT:(sim/cockpit/engine/idle_speed[0]:0)&&(sim/cockpit/engine/idle_speed[1]:0)
sw_item: BATT 1 / BATT 2 Switches|ON:(sim/cockpit2/electrical/battery_on[0]:1)&&(sim/cockpit2/electrical/battery_on[1]:1)
sw_item: DC Voltage (Min. 22V DC)|CHECK:sim/cockpit2/electrical/bus_volts[0]:>22
sw_item: Beacon Light|ON:sim/cockpit2/switches/beacon_on:1
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_item: Cabin Signs|BOTH:(sim/cockpit/switches/fasten_seat_belts:1)&&(sim/cockpit/switches/no_smoking:1)
sw_item: Electric Master Auxiliary Power|OFF:sim/cockpit/electrical/generator_apu_on:0
sw_item: APU Master Switch|ON:sim/cockpit/engine/APU_switch:1
sw_item: Left Main Fuel Boost Pump|ON:sim/cockpit/engine/fuel_pump_on[0]:1
sw_item: APU Start Switch|PRESS:sim/cockpit/engine/APU_switch:2
sw_item: APU RPM|CHECK (97% - 103%):sim/cockpit/engine/APU_N1:97|103
sw_item: EGT|MAX. 988°C
sw_itemvoid:
sw_itemvoid: CAUTION
sw_itemvoid: IF APU FAILS TO COME UP TO SPEED OR START
sw_itemvoid: SWITCH LIGHTREMAINS ILLUMINATED, DEPRESS
sw_itemvoid: OVERSPEED TEST-SWITCH.  IF APU STARTSWITCH
sw_itemvoid: LIGHT STILL REMAINS ILLUMINATED, PLACE APU 
sw_itemvoid: MASTER SWITCH AND BATTERY SWITCHES 1 AND 2
sw_itemvoid: OFF.
sw_itemvoid:
sw_itemvoid:             1 of 15 - Next BEFORE STARTING ENGINES


sw_checklist: BEFORE STARTING ENGINES (1/2):Before Starting Engines
sw_item: Preflight Checklists|COMPLETE
sw_item: Parking Brake|SET:sim/flightmodel/controls/parkbrake:1
sw_item: ELECTRIC MASTER LEFT PWR / RIGHT PWR Switches|OFF:(sim/cockpit/electrical/generator_on[0]:0)&&(sim/cockpit/electrical/generator_on[1]:0)
sw_item: BATT 1 / BATT 2 Switches|ON:(sim/cockpit2/electrical/battery_on[0]:1)&&(sim/cockpit2/electrical/battery_on[1]:1)
sw_item: Essential AC / DC Bus Volts:(sim/cockpit2/electrical/bus_volts[0]:22|27)&&(sim/cockpit2/electrical/bus_volts[1]:22|27)
sw_itemvoid: - DC Voltage 22 VDC to 27 VDC
sw_itemvoid: - AC Frequency 400 HZ
sw_itemvoid: - AC Voltage 115 VAC|CHECK
sw_item: HP Fuel Cocks|SHUT:(sim/cockpit/engine/idle_speed[0]:0)&&(sim/cockpit/engine/idle_speed[1]:0)
sw_item: ELECTRICAL AUX POWER|ON:sim/cockpit/electrical/generator_apu_on:1
sw_item: DISPLAY Switches (3)|ON:sim/cockpit2/radios/indicators/nav1_display_horizontal:1
sw_item: CABIN / GALLEY / RADIO MASTER Switches|ON:(sim/cockpit2/switches/generic_lights_switch[2]:1)&&(sim/cockpit2/switches/generic_lights_switch[3]:1)
sw_item: Display Controllers|ON
sw_item: FMS|INITIALZE
sw_item: DISPLAY SWITCHING / SYMBOL GENERATOR CONTROL|NORM
sw_item: PRESSURIZATION CONTROL|CHECK / SET
sw_item: ANTI-ICE Switches (4)|OFF:(sim/cockpit/switches/anti_ice_AOA_heat:0)&&(sim/cockpit2/ice/ice_pitot_heat_on_pilot:0)&&(sim/cockpit2/ice/ice_pitot_heat_on_copilot:0)&&(sim/cockpit/switches/anti_ice_window_heat:0)
sw_item: FUEL SYSTEM|CHECK
sw_item: ENGINE START SWITCHES (2)|OFF:(sim/cockpit2/engine/actuators/starter_hit[0]:0)&&(sim/cockpit2/engine/actuators/starter_hit[1]:0)
sw_itemvoid: EXTERIOR LIGHTS|AS REQUIRED
sw_itemvoid: ANTI ICE HTR Switches|AS REQUIRED
sw_item: AUX PUMP / Brake System|CHECK
sw_itemvoid: COCKPIT LIGHTS|AS REQUIRED
sw_item: Warning Lights|CHECK
sw_itemvoid:
sw_itemvoid:             2 of 15 - Next BEFORE STARTING ENGINES (2/2)


sw_checklist: BEFORE STARTING ENGINES (2/2)
sw_itemvoid:======================
sw_itemvoid:      INSTRUMENT PANEL
sw_itemvoid:======================
sw_item: Clocks|CHECK
sw_item: Display Controllers|CHECK
sw_item: Altimeters|SET / CROSS CHECKED
sw_item: Flight Guidance Panel|CHECK
sw_item: Thrust Reverser Lights|CHECK
sw_item: Fuel Quantity (Normal and Standby)|TEST
sw_item: Cabin Pressurization Controller|SET
sw_item: Flap Indicator|CHECK
sw_item: Landing Gear Handle|DOWN / 3 GREEN:sim/cockpit2/controls/gear_handle_down:1
sw_itemvoid:======================
sw_itemvoid:      CENTER PEDESTAL
sw_itemvoid:======================
sw_item: Fire Handles|IN:(sim/cockpit2/engine/actuators/fire_extinguisher_on[0]:0)&&(sim/cockpit2/engine/actuators/fire_extinguisher_on[1]:0)
sw_item: Power Levers|IDLE:sim/cockpit2/engine/actuators/throttle_ratio_all:0
sw_item: SPEED BRAKE Handle|RETRACT:sim/cockpit2/controls/speedbrake_ratio:0
sw_item: Elevator Trim|CHECK / SET:sim/cockpit2/controls/elevator_trim:-0.10|0.05
sw_item: GND SPLR Switch|OFF:sim/cockpit2/controls/speedbrake_ratio:0
sw_item: PARK/EMERG BRAKE Handle|ON:sim/flightmodel/controls/parkbrake:1
sw_item: Radios|SET
sw_item: Rudder and Aileron Trim (see QRH pg. 5)|CHECK
sw_itemvoid:
sw_itemvoid:             3 of 15 - Next STARTING ENGINES


sw_checklist: STARTING ENGINES (1/2):Starting Engines
sw_item: Start Page|SELECT
sw_item: HP Fuel Cocks|SHUT:(sim/cockpit/engine/idle_speed[0]:0)&&(sim/cockpit/engine/idle_speed[1]:0)
sw_item: POWER Levers|IDLE:sim/cockpit2/engine/actuators/throttle_ratio_all:0
sw_item: Beacon Light|ON:sim/cockpit2/switches/beacon_on:1
sw_item: Fuel Boost Pumps (One Each Side)|ON / MESSAGE OUT:(sim/cockpit/engine/fuel_pump_on[0]:1)&&(sim/cockpit/engine/fuel_pump_on[1]:1)
sw_item: Electrical Power|CHECK (Max. 35%)
sw_item: Engine Start Master|ON:sim/cockpit/engine/ignition_on[2]:3
sw_itemvoid:======================
sw_itemvoid:      RIGHT ENGINE
sw_itemvoid:======================
sw_item: Engine Start Switch|PRESS:sim/cockpit2/engine/actuators/starter_hit[1]:1
sw_item: Start Valve and Ignition|ON:sim/cockpit/warnings/annunciators/igniter_on[1]:1
sw_item: Positive LP RPM|CHECK
sw_item: HP Fuel Cock|OPEN (Min. 15% HP):sim/cockpit/engine/idle_speed[1]:1
sw_item: Start Valve and Ignition|OFF:sim/cockpit/warnings/annunciators/igniter_on[1]:0
sw_item: TGT|MONITOR (Max. 700°C):sim/flightmodel/engine/ENGN_ITT_c[1]:<700
sw_item: Engine RPM|CHECK (Min. 46.6% HP):sim/cockpit2/engine/indicators/N2_percent[1]:>46.6
sw_item: Oil Pressure and Temperature|CHECK
sw_item: EVM|CHECK
sw_itemvoid: Hydraulic Pressure (COMB/FLT/UTIL/AUX)|CHECKED (0/3000/3000/0)
sw_itemvoid: Note: actual values are different!
sw_itemvoid:
sw_itemvoid:             4 of 15 - Next STARTING ENGINES (2/2)

sw_checklist: STARTING ENGINES (2/2)
sw_itemvoid:======================
sw_itemvoid:      LEFT ENGINE
sw_itemvoid:======================
sw_item: Engine Start Switch|PRESS:sim/cockpit2/engine/actuators/starter_hit[0]:1
sw_item: Start Valve and Ignition|ON:sim/cockpit/warnings/annunciators/igniter_on[0]:1
sw_item: Positive LP RPM|CHECK
sw_item: HP Fuel Cock|OPEN (Min. 15% HP):sim/cockpit/engine/idle_speed[0]:1
sw_item: Start Valve and Ignition|OFF:sim/cockpit/warnings/annunciators/igniter_on[0]:0
sw_item: TGT|MONITOR (Max. 700°C):sim/flightmodel/engine/ENGN_ITT_c[0]:<700
sw_item: Engine RPM|CHECK (Min. 46.6% HP):sim/cockpit2/engine/indicators/N2_percent[0]:>46.6
sw_item: Oil Pressure and Temperature|CHECK
sw_item: EVM|CHECK
sw_itemvoid: Hydraulic Pressure (COMB/FLT/UTIL/AUX)|CHECKED (3000/3000/0/0)
sw_itemvoid: Note: actual values are different!
sw_itemvoid:
sw_itemvoid:             5 of 15 - Next AFTER STARTING ENGINES


sw_checklist: AFTER STARTING ENGINES:After starting engines
sw_item: Start Master|OFF:sim/cockpit/engine/ignition_on[2]:0
sw_item: ELECTRIC MASTER LEFT / RIGHT PWR Switches|ON:(sim/cockpit/electrical/generator_on[0]:1)&&(sim/cockpit/electrical/generator_on[1]:1)
sw_item: Battery Ammeters|CHECK
sw_item: Doors|CLOSED:sim/cockpit2/switches/custom_slider_on:0
sw_item: Anti-Ice Heat Switches|ON:(sim/cockpit/switches/anti_ice_AOA_heat:1)&&(sim/cockpit2/ice/ice_pitot_heat_on_pilot:1)&&(sim/cockpit2/ice/ice_pitot_heat_on_copilot:1)&&(sim/cockpit/switches/anti_ice_window_heat:1)
sw_itemvoid: Cowl / Wing Anti-ice Switches|CHECK / AS REQUIRED
sw_item: Pressurization Control|AUTO / FLIGHT / SET
sw_item: Fuel Boost Pumps / Crossflow Valve|ON / CLOSE:(sim/cockpit/engine/fuel_pump_on[0]:1)&&(sim/cockpit/engine/fuel_pump_on[1]:1)
sw_item: Ground Spoilers|CHECK
sw_item: Flight Controls / Bungee / Rudder Torque Limiter|CHECK
sw_item: Yaw Damper|ON:sim/cockpit/switches/yaw_damper_on:1
sw_itemvoid:
sw_itemvoid:             6 of 15 - Next TAXI / BEFORE TAKE-OFF


sw_checklist: TAXI / BEFORE TAKE-OFF:Taxi / Before Take-Off
sw_item: Transponder|SET / STANDBY:sim/cockpit/radios/transponder_mode:1
sw_item: Taxi Light|ON:sim/cockpit2/switches/taxi_light_on:1
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_itemvoid: Cowl / Wing Anti-Ice|AS REQUIRED
sw_item: Parking Brake|RELEASED:sim/flightmodel/controls/parkbrake:0
sw_item: Brakes|CHECK:(sim/cockpit2/controls/left_brake_ratio:1)&&(sim/cockpit2/controls/right_brake_ratio:1)
sw_item: Slip Indicators / Compasses / Flight Instruments|CHECK
sw_item: Thrust Reversers Operational Check|COMPLETE:(sim/flightmodel2/engines/thrust_reverser_deploy_ratio[0]:>0.9)&&(sim/flightmodel2/engines/thrust_reverser_deploy_ratio[1]:>0.9)
sw_item: Thrust Reverser Lights|CHECK
sw_itemvoid: - REV ARM|ON
sw_itemvoid: - REV UNLOCK / REV DEPLOY|OUT
sw_itemvoid:   NOTE
sw_itemvoid:   If either or both UNLOCK or DEPLOY lights are
sw_itemvoid:   ON, maintenance is required before flight.
sw_item: Fuel Temperature|CHECK
sw_item: Crew Briefing / EPR / V Speeds|BRIEFED
sw_item: Trim Settings (3)|SET
sw_item: Flaps / Stabilizer|SET TAKE-OFF:sim/flightmodel/controls/flaprqst:0.666667
sw_item: Engine Instruments|CHECK
sw_item: Hydraulic Pressure (COMB/FLT/UTIL/AUX)|CHECKED (3000/3000/0/0)
sw_itemvoid: Note: actual values are different!
sw_itemvoid: APU|AS DESIRED
sw_item: Flight Guidance Panel|SET
sw_itemvoid:
sw_itemvoid:             7 of 15 - Next LINE-UP


sw_checklist: LINE-UP:Line-up
sw_item: Parking Brake|SET:sim/flightmodel/controls/parkbrake:1
sw_item: Strobe Light|ON:sim/cockpit2/switches/strobe_lights_on:1
sw_item: Landing Lights|ON:sim/cockpit2/switches/landing_lights_on:1
sw_item: Taxi Light|OFF:sim/cockpit2/switches/taxi_light_on:0
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_item: Ground Spoilers|ARMED:sim/cockpit2/controls/speedbrake_ratio:-0.5
sw_item: Transponder|ON:sim/cockpit/radios/transponder_mode:3
sw_item: TCAS|ON:sim/cockpit2/EFIS/EFIS_tcas_on:1
sw_itemvoid: Autothrottle|ARM / ENGAGED (IF DESIRED)
sw_item: Departure Runway Alignment|BOTH PILOTS CONFIRM
sw_item: Parking Brake|RELEASED:sim/flightmodel/controls/parkbrake:0
sw_itemvoid:
sw_itemvoid:             8 of 15 - Next CLIMB


sw_checklist: CLIMB:Climb
sw_item: Landing Gear|UP:sim/cockpit2/controls/gear_handle_down:0
sw_item: Flaps|UP:sim/flightmodel/controls/flaprqst:0
sw_itemvoid: Limit bank angle to 15 degrees while the
sw_itemvoid: flaps are retracting until reaching a
sw_itemvoid: speed greater than VREF on the speed tape.
sw_item: Flight Guidance Panel|SET
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_item: Ignition|OFF:(sim/cockpit/warnings/annunciators/igniter_on[0]:0)&&(sim/cockpit/warnings/annunciators/igniter_on[1]:0)
sw_item: Ground Spoilers|OFF:sim/cockpit2/controls/speedbrake_ratio:0
sw_item: Pressurization|CHECK
sw_itemvoid: Engine Climb Power / Autothrottle|SET / AS REQUIRED
sw_itemvoid: Engine Synchronizer|AS REQUIRED
sw_item: Altimeters (3) (AT TRANSITION ALTITUDE)|SET & CROSS-CHECKED
sw_item: Landing Lights|OFF (ABOVE 10.000 FT):sim/cockpit2/switches/landing_lights_on:0
sw_item: APU|SHUT DOWN PRIOR TO 30.000 FT:sim/cockpit/engine/APU_switch:0
sw_itemvoid:
sw_itemvoid:             9 of 15 - Next CRUISE


sw_checklist: CRUISE:Cruise
sw_itemvoid: Power|SET FOR CRUISE
sw_itemvoid: Pressurization|CHECK
sw_itemvoid: Cabin Signs|AS REQUIRED
sw_itemvoid: Panel Sweep|COMPLETE
sw_itemvoid: NOTE
sw_itemvoid: A panel sweep or a check for normal
sw_itemvoid: system operation and indication
sw_itemvoid: should be accomplished at top-of-climb,
sw_itemvoid: top-of-descent, and at regular intervals
sw_itemvoid: between top-of-climb and top-of-descent.
sw_itemvoid:
sw_itemvoid:             10 of 15 - Next DESCENT


sw_checklist: DESCENT:Descent
sw_itemvoid: Crew Briefing (VREF / Go-Around Power)|BRIEFED
sw_item: Cabin Signs|BOTH:(sim/cockpit/switches/fasten_seat_belts:1)&&(sim/cockpit/switches/no_smoking:1)
sw_item: FMS|ARRIVAL SET
sw_item: Flight Instruments|SET / AS REQUIRED
sw_itemvoid: - NAV AIDS|TUNED AND IDENTIFIED
sw_itemvoid: - Course Selection|INBOUND COURSE
sw_itemvoid: Cowl / Wing Anti-Ice|AS REQUIRED
sw_item: Pressurization|SET
sw_item: Fuel Boost Pumps|ON:(sim/cockpit/engine/fuel_pump_on[0]:1)&&(sim/cockpit/engine/fuel_pump_on[1]:1)
sw_item: Parking Brake|RELEASED:sim/flightmodel/controls/parkbrake:0
sw_item: Landing Lights|ON (BELOW 10.000 FT):sim/cockpit2/switches/landing_lights_on:1
sw_itemvoid:
sw_itemvoid:             11 of 15 - Next APPROACH


sw_checklist: APPROACH:Approach
sw_item: Altimeters (3) (AT TRANSITION LEVEL)|SET & CROSS-CHECKED
sw_itemvoid: Flaps|AS REQUIRED
sw_item: VREF / Go-Around Power|CHECKED
sw_item: Hydraulic Pressure (COMB/FLT/UTIL/AUX)|CHECKED (3000/3000/0/0)
sw_itemvoid: Note: actual values are different!
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_itemvoid:
sw_itemvoid:             12 of 15 - Next BEFORE LANDING


sw_checklist: BEFORE LANDING:Before Landing
sw_item: Landing Gear|DOWN / 3 GREEN:sim/cockpit2/controls/gear_handle_down:1
sw_item: Crew Alerting System|CHECK
sw_item: Ground Spoilers|ARMED:sim/cockpit2/controls/speedbrake_ratio:-0.5
sw_itemvoid: NOTE
sw_itemvoid: If touch and go landing is to be performed,
sw_itemvoid: GND SPLR should be OFF for this maneuver. 
sw_itemvoid: Manual spoiler landing distance should be 
sw_itemvoid: taken into account.
sw_itemvoid:
sw_item: Flaps|SET FOR LANDING:sim/flightmodel/controls/flaprqst:1
sw_itemvoid: CAUTION
sw_itemvoid: DO NOT MOVE REVERSE THRUST LEVERS
sw_itemvoid: OUT OF THE FORWARD POSITION PRIOR
sw_itemvoid: TO TOUCHDOWN.
sw_itemvoid:
sw_itemvoid: NOTE
sw_itemvoid: Maintain a minimum 67% HP RPM until landing.
sw_itemvoid:
sw_itemvoid:             13 of 15 - Next AFTER LANDING


sw_checklist: AFTER LANDING:After Landing
sw_item: Taxi Light|ON:sim/cockpit2/switches/taxi_light_on:1
sw_item: Landing Lights|OFF:sim/cockpit2/switches/landing_lights_on:0
sw_item: Strobe Light|OFF:sim/cockpit2/switches/strobe_lights_on:0
sw_item: Ignition|OFF:(sim/cockpit/warnings/annunciators/igniter_on[0]:0)&&(sim/cockpit/warnings/annunciators/igniter_on[1]:0)
sw_itemvoid: Transponder|AS REQUIRED
sw_item: Flaps|UP:sim/flightmodel/controls/flaprqst:0
sw_itemvoid: COWL / WING ANTI-ICE / ANTI-ICE HTRS|AS REQUIRED / OFF
sw_item: Fuel Boost Pumps|OFF:(sim/cockpit/engine/fuel_pump_on[0]:0)&&(sim/cockpit/engine/fuel_pump_on[1]:0)
sw_item: Ground Spoilers|OFF:sim/cockpit2/controls/speedbrake_ratio:0
sw_itemvoid: APU|AS REQUIRED
sw_itemvoid:
sw_itemvoid:             14 of 15 - Next SHUTDOWN


sw_checklist: SHUTDOWN:Shutdown
sw_item: Parking Brake|ON:sim/flightmodel/controls/parkbrake:1
sw_item: Transponder|STANDBY:sim/cockpit/radios/transponder_mode:1
sw_item: ELECTRIC MASTER LEFT PWR / RIGHT PWR Switches|OFF:(sim/cockpit/electrical/generator_on[0]:0)&&(sim/cockpit/electrical/generator_on[1]:0)
sw_item: HP Fuel Cocks|SHUT:(sim/cockpit/engine/idle_speed[0]:0)&&(sim/cockpit/engine/idle_speed[1]:0)
sw_item: Radios|OFF
sw_itemvoid: Exterior Lights|AS REQUIRED
sw_item: Fuel Boost Pumps|OFF:(sim/cockpit/engine/fuel_pump_on[0]:0)&&(sim/cockpit/engine/fuel_pump_on[1]:0)
sw_itemvoid: Cockpit Lights|AS REQUIRED
sw_item: Display Units|OFF:sim/cockpit2/radios/indicators/nav1_display_horizontal:0
sw_item: CABIN / GALLEY / RADIO MASTER Switches|OFF:(sim/cockpit2/switches/generic_lights_switch[2]:0)&&(sim/cockpit2/switches/generic_lights_switch[3]:0)
sw_item: ELECTRIC MASTER AUX PWR|OFF:sim/cockpit/electrical/generator_apu_on:0
sw_item: APU|OVERSPEED / TEST:sim/cockpit/engine/APU_switch:0
sw_item: BATT 1 / BATT 2 Switches|OFF:(sim/cockpit2/electrical/battery_on[0]:0)&&(sim/cockpit2/electrical/battery_on[1]:0)
sw_itemvoid:
sw_itemvoid: ===============================
sw_itemvoid:      Good bye and enjoy a nice cup of coffee...
sw_itemvoid: ===============================
sw_itemvoid:
sw_itemvoid:             15 of 15 - END
